{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":28,"n_cols":13,"rows_kept":28,"cut":false,"hidden":false,"merged":[[25,2,25,6],[26,2,26,6],[16,6,16,10],[17,6,17,10],[18,6,18,10],[19,1,19,5],[17,1,17,5],[25,7,25,13],[20,1,20,5],[22,6,22,10],[0,1,0,9],[25,0,25,1],[26,0,26,1],[27,0,27,1],[24,0,24,1],[17,11,17,13],[19,6,19,10],[27,2,27,6],[22,1,22,5],[6,1,6,2],[19,11,19,13],[15,11,15,13],[12,9,12,13],[8,3,8,5],[13,3,14,8],[18,1,18,5],[16,1,16,5],[15,1,15,5],[13,9,13,13],[14,9,14,13],[11,3,12,8],[11,9,11,13],[7,1,7,2],[8,1,8,2],[27,7,27,13],[23,11,23,13],[16,11,16,13],[18,11,18,13],[20,11,20,13],[21,11,21,13],[22,11,22,13],[26,7,26,13],[20,6,20,10],[21,6,21,10],[23,6,23,10],[24,7,24,13],[24,2,24,6],[21,1,21,5],[23,1,23,5],[8,12,8,13],[9,3,9,13],[10,3,10,8],[15,6,15,10],[10,9,10,13],[7,3,7,5],[7,8,7,9],[7,10,7,11],[7,12,7,13],[8,8,8,9],[8,10,8,11],[4,1,4,2],[6,12,6,13],[4,8,4,9],[4,10,4,11],[4,12,4,13],[5,12,5,13],[6,3,6,5],[5,3,5,5],[5,8,5,9],[5,10,5,11],[1,1,1,2],[1,3,1,12],[2,1,2,2],[2,3,2,13],[5,1,5,2],[6,8,6,9],[6,10,6,11],[3,1,3,2],[3,3,4,5],[3,6,3,13]],"flags":["formulas_cached_only"]}
[null,"Activity Hazard Analysis (AHA)"]
["Activity/Work Task: ","Gypsum Board: Finishing",null,"Overall Risk Assessment Code (RAC) (Use highest code) "]
["Project Location: ",null,null,"Risk Assessment Code (RAC) Matrix "]
["Contract Number: ",null,null,"Severity ",null,null,"Probability "]
["Date Prepared: ",{"$nulls":5},"Frequent ","Likely ","Occasional ",null,"Seldom ",null,"Unlikely "]
["Prepared by (Name/Title): ","Chris Kirby",null,"Catastrophic ",null,null,"E ","E ","H ",null,"H ",null,"M "]
[null,"President",null,"Critical ",null,null,"E ","H ","H ",null,"M ",null,"L "]
["Reviewed by (Name/Title): ",null,null,"Marginal ",null,null,"H ","M ","M ",null,"L ",null,"L "]
[null,null,null,"Negligible ",null,null,"M ","L ","L ",null,"L ",null,"L "]
["Notes: (Field Notes, Review Comments, etc.) ",null,null,"Step 1: Review each “Hazard” with identified safety “Controls” and determine RAC (See above) "]
[null,null,null,"“Probability” is the likelihood to cause an incident, near miss, or accident and identified as: Frequent, Likely, Occasional, Seldom or Unlikely. ",{"$nulls":5},"RAC Chart "]
[null,null,null,"“Severity” is the outcome/degree if an incident, near miss, or accident did occur and identified as: Catastrophic, Critical, Marginal, or Negligible  ",{"$nulls":5},"E = Extremely High Risk "]
[{"$nulls":9},"H = High Risk "]
[null,null,null,"Step 2: Identify the RAC (Probability/Severity) as E, H, M, or L for each “Hazard” on AHA. Annotate the overall highest RAC at the top of AHA.  ",{"$nulls":5},"M = Moderate Risk "]
[{"$nulls":9}," L = Low Risk "]
["Job Steps ","Hazards ",{"$nulls":4},"Controls ",{"$nulls":4},"RAC "]
["1.  Material storage and handling","Tripping, falling, inadequate passageway, fire in lumber storage areas.",{"$nulls":4},"Maintain safe storage areas with proper aisle clearance between rows of metal studs, drywall, and rough carpentry materials.  Keep materials covered and unexposed to weather.  Use gloves when handling stored items.  Bend knees when carrying pails to decrease possiblity of back injury.  Use equipment to move materials safely. Fire extinguisher to be provided at intermediate intervals.",{"$nulls":4},"L"]
["2.  Equipment / Tool Usage","Cuts, eye injuries, contusions, excess noise from Chop saws and PAT’s, electrical shock.  Ricochet from PAT’s.",{"$nulls":4},"All equipment to be safety checked prior to start up.  Personal protective equipment to be worn as necessary for the work at hand.  Guards to be in place on all power tools and not removed or rendered inoperable.  Power cords to be in proper working condition.   Proper eye and ear protection will be used at all times during usage.   No smoking during activity.  Only OSHA approved gas containers to be used on the job and must be stored a minimum of 10’ from equipment.  Fire extinguishers to be kept a minimum of 8’ from equipment.  ",{"$nulls":4},"L"]
["3.  Drywall Finishing","Trips, falls, dust in eyes, cuts from razors.",{"$nulls":4},"After walls have received drywall screwed to studs and track. Precaution to be taken when opening pails of joint compound and cutting of trim items.  Proper work boots to be worn-no tennis shoes or open toed shoes allowed.  Hard hats and eye protection to be worn at all times.  Gloves to be worn as necessary.  Work areas to be kept neat and clean.  Scrap materials to be disposed properly, daily.  Use of dust masks is mandatory when sanding.  ",{"$nulls":4},"M"]
["4.  Operation of Equipment","Untrained operators, defective equipment, injured personnel slipping/falling off equipment, incipient fires.",{"$nulls":4},"Only qualified persons shall be assigned as operators.  Equipment checklists shall be maintained and followed.  Equipment must be checked daily for safety compliance and serviced on a regular basis.  Operator shall never leave machine or make repairs while it is still running or mobile.  Climbing on and off while equipment is running is prohibited.  Seat belts shall be used at all times.  Equipment to be kept free of mud, grease, oil, etc.  Only operator allowed on any part of the equipment.  Running boards and steps to be provided with non-slip surfaces.  No tools shall be left lying on any part of equipment.  All equipment to have at least one fire extinguisher rated 5BC.",{"$nulls":4},"M"]
["5.  Emergency Help","Choking, minor injuries, first aid, etc.",{"$nulls":4},"First aid facilities are located at the Jobsite Trailer and Superintendent vehicles.  At least one employee will be certified in CPR and First Aid.  Report all accidents immediately.",{"$nulls":4},"L"]
["6.  Training","Safety / Health / Accident Prevention",{"$nulls":4},"Employees will review Safety Handbook.",{"$nulls":4},"L"]
["7.  Hazard Communication Standard","Potential exposure to hazardous material.",{"$nulls":4},"All shipments of products considered hazardous under HazCom must be properly labeled and accompanied by the appropriate Material Safety Data Sheet (MSDS).  All employees will be trained in the “Right to Know” Standard, understand MSDS forms and labeling, safety measures, and have access to all MSDS’s.",{"$nulls":4},"L"]
["8.  Housekeeping","Tripping, littering, pollution, rodents, insects, fire.",{"$nulls":4},"All debris to be put in dumpster on a continuous basis to avoid debris blowing around project.  Lunch/snack scraps shall be put in dumpster immediately after break.",{"$nulls":4},"L"]
["Equipment to be Used ",null,"Training Requirements/Competent or Qualified Personnel name(s) ",{"$nulls":4},"Inspection Requirements "]
["Mixing Drill, Ladder, Mud Pan & Knife;",null,"Competent/Qualified Personnel:",{"$nulls":4},"Inspect Guards and Cords Daily"]
["Power Cords; Scissor Lifts",null,"OSHA Construction Safety & Health, First Aid, CPR, Power Actuated Tools, Aerial Lifts, Scaffolding/Lift Inspection",{"$nulls":4},"Inspect Scaffolding & Lifts Daily"]
[{"$nulls":7},"Inspect First Aid Kits Monthly"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}